


WLAN Software RELEASE NOTES

WLAN Software Version 3.4.7.33
October 28, 2003
INTRODUCTION:
This product is an 802.11 wireless station in Cardbus/miniPCI/PCI/USB interface. The software will install the WlanUtility/APUtility and driver to user computer. The supported OS contains Windows 98SE/ME/2000/XP.
History:
	Status
	Version No.
	Release Date
	History

	Current Version
	3.4.7.33
	10/28/2003
	Driver version 3.30.15.0( MS6802/04/07/19/20/25)

1.69.3731.2003 (MS6823)

1.10.0.0 (MS6827/28/29, 1.10.1.0 for Win2K)
2.9.8.345 (MS6978)

1.0.17.65(MS6818)
0.9.0.0(MS6826)
WlanUtility version 2.11.37.64
APUtility version 2.2.2.24

	Previous Version
	3.4.6.32
	10/17/2003
	Driver version 3.30.15.0( MS6802/04/07/19/20/25)

1.69.3731.2003 (MS6823)

1.9.0.0 (MS6827/28/29)

2.9.8.345 (MS6978)

1.0.17.65(MS6818)
0.9.0.0(MS6826)
WlanUtility version 2.11.37.64
APUtility version 2.2.1.24

	Previous Version
	3.4.6.31
	10/1/2003
	Driver version 3.30.15.0( MS6802/04/07/19/20/25)

1.69.3731.2003 (MS6823)

1.9.0.0 (MS6827/28/29)

2.9.8.345 (MS6978)

1.0.17.65(MS6818)
0.9.0.0(MS6826)
WlanUtility version 2.11.36.63
APUtility version 2.2.1.23

	Previous Version
	3.3.6.30
	9/22/2003
	Driver version 3.30.15.0( MS6802/04/07/19/20/25)

1.69.3731.2003 (MS6823)

1.9.0.0 (MS6827/28/29)

2.9.8.345 (MS6978)

1.0.17.65(MS6818)

Utility version 2.10.36.62

APUtility version 2.1.1.22


SUPPORTED Feature
Station mode

	Features
	Comment

	XP Zero Configuration UI
	

	Channel display and setting  (not in infrastructure mode)
	

	Speed display and setting
	

	Radio On/Off display and setting
	

	MAC address display
	

	IP address display
	

	Transmit packets display
	

	Received packets display
	

	Signal strength display
	

	Link quality display
	

	Visible network display
	

	Selected network standard display
	

	Selected network supported rates display
	

	Fragmentation threshold display and setting
	

	RTS threshold display and setting
	

	Locale display and setting
	Yes(MS6823/MS6978 don’t support)

	Power save mode display and setting
	

	Card model display
	

	Driver version display
	

	Utility version
	

	Utility build date
	

	Multi-Language support
	Traditional(Simplified) Chinese, English, Germany, French, Japan

	Multi-card support
	


AP/Gateway mode (Windows XP)
	Features
	Comment

	LAN
	

	DHCP Server
	

	Static IP
	

	UPnP 
	

	WAN 
	(Gateway mode, depends on hardware)

	Static IP
	

	DHCP Client
	

	PPPoE
	Need another ethernet card

	PPTP
	

	Direct Link
	

	Wireless
	

	Radio & Channel setting
	

	Data Rate
	

	64/128 bits WEP
	

	Association Control & List
	

	Gateway
	

	NAT – ALGs (FTP, ICMP, TELNET, HTTP, NNTP, SMTP, Messenger)
	

	VPN Passthrough (PPTP)
	

	Remote Management (http port 8080)
	

	Password Management
	

	Status and Statistics
	

	Reset Factory Default
	


SUPPORTED HardWAre
	Board Type
	Description

	MS6802
	802.11b Cardbus

	MS6804
	802.11b miniPCI

	MS6807
	802.11b PCI

	MS6818
	802.11g miniPCI (no AP/Gateway mode)

	MS6819
	802.11g Cardbus

	MS6820
	802.11g miniPCI

	MS6823
	802.11b USB 

	MS6825
	802.11g PCI

	MS6826
	802.11g USB(2.0) (no AP/Gateway mode)

	MS6827
	802.11b mini-PCI

	MS6828
	802.11b PCI

	MS6829
	802.11b Cardbus

	MS6978
	802.11b USB (No AP/Gateway mode support)


Installation Notes:
miniPCI/PCI
1. Place the hardware into PC/Laptop

2. After reboot, if System prompts “New Hardware Finding Wizard”, just click “Cancel”.

3. Double click Setup.exe and fill in necessary information,  setup wizard will all things for you.
USB/Cardbus

1. Double click Setup.exe and fill in necessary information.

2. Plug-in hardware after installation

3. If system prompts “New Hardware Finding Wizard”, just click “Next” and system will automatically finish it.
Uninstall

1. Please make sure the hardware is in PC.

2. Select uninstall in “Start” => “Programs” => “IEEE 802.11 Wireless LAN Software”
3. Select “Yes” and uninstall program will finish it automatically.
Re-install

1. Place the hardware into PC/Laptop. (Note: During the uninstall and install process, do not remove hardware from your PC/Laptop)

2. Select uninstall in “Start” => “Programs” => “IEEE 802.11 Wireless LAN Software”
3. Double click Setup.exe and fill in necessary information.

Configuration Notes:
Under Windows 98SE/ME/2000,

WlanUtility will auto-start when system boot. The user could use WlanUtility to connect to available network.

Under XP,

XP will use build-in Zero Configuration to connect to available network.  But if the user wants to use WlanUtility, he has to uncheck “Use windows to configure my wireless network settings” to make WlanUtility work.

Software AP( Windows XP only)

Right click wireless icons in the system tray and select “Switch to AP mode”.  APUtility will automatically join all network cards into the bridge and turn WLAN cards into AP mode. If the user wants to change AP mode configuration, he can link to http://localhost:8080 and the default user name and password is both “admin”.
Software Gateway( Windows XP only)

Right click wireless icons in the system tray and select “Switch to Gateway mode”.  APUtility will pop-up an IP sharing dialog.  Choose your WAN connection (If you did not create yet, please create it first), APUtility will do the NAT translation between WAN and wireless. If the user wants to change AP mode configuration, he can link to http://localhost:8080 and the default user name and password is both “admin”.
Changes and Enhancements:
Installation 3.4.7.33

1. Fix MS6823 can’t delete association control list problem

2. MS6827/28/29 Windows 2000/XP WHQL certified

Installation 3.4.6.32
1.      Fix SSID length = 32 will cause profile management working incorrectly problem.
2.      Fix renew IP process too slow problem under win 2000.
3.      Link to APs without broadcast SSID.
4.      Change board name to marketing name.
Installation 3.4.6.31

1. AP/Gateway mode support for MS6823.
2. MS6826 XP/2000 support (Still in Beta driver 0.9.0.0).
3. In gateway mode, no LAN IP setting available now because XP doesn’t allow to change IP other than 192.168.0.1.
4. MS6802/04/07/19/20/25 driver 3.30.15.0 XP/2000 WHQL certified.
5. Fix MS6802/04/07/19/20/25 auto-connect too slow problem when hardware radio off/on again.

6. Add channel recommend to MS6802/04/07/19/20/25 in AP/Gateway mode.

7. Japan Language support.

Installation 3.3.6.30

1. Drivers of MS6827/28/29 changes to 1.9.0.0

2. Translate some gateway mode words to Germany and Simplified Chinese

Installation 3.3.5.30
1. First introduce the One-Installation Feature

2. Add Gateway support

3. Change the http port from 80 to 8080
Limitations:
1. (STA)When data rates in (g only), only g APs could be found.

2. (AP/Gateway) User could only change password, not user name.
3. (AP/Gateway) no multi-card supported now, APUtility will use the first founded card as its wireless side.
4. Don’t support XP switching user features, please logout then login as different user.
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