


MSI WLAN Software RELEASE NOTES

MSI WLAN Software Version 1.0.0.0302
March 2, 2006
INTRODUCTION:
This product is an 802.11 wireless station in Cardbus/miniPCI/PCI/USB interface. The software will install the MSI WlanUtility and driver to user computer. The supported OS contains Windows XP64BT.

History:
	Status
	Version No.
	Release Date
	History

	Current Version
	1.0.0.0302
	3/2/2006
	Driver version

3.1.0.0 (MS6833/33A/34/35/55B)

2.0.4.0 (MS6861/65)

1.0.4.0 (MS6833B/34B)
1.0.4.0 (MS-6877)
WlanUtility version 1.0.0.0302
WlanService version 1.0.0.0302


SUPPORTED Feature
Station mode

	Features
	Comment

	Channel display and setting  (not in infrastructure mode)
	

	Speed display and setting
	

	Radio On/Off display and setting
	

	MAC address display
	

	IP address display
	

	Transmit packets display
	

	Received packets display
	

	Signal strength display
	

	Link quality display
	

	Visible network display
	

	Fragmentation threshold display and setting
	

	RTS threshold display and setting
	

	Locale display and setting
	

	Power save mode display and setting
	

	Driver version display
	

	Utility version
	

	Multi-Language support
	Traditional(Simplified) Chinese, English, Germany, French, Japan

	Multi-card support
	PCI /mini PCI/USB


Authentication
	Features
	Comment

	MD5-Challenge (Authentication)
	MS6833/33A/33B/34/34B/35/55B/61/65/77

	LEAP (Authentication)
	MS6833/33A/33B/34/34B/35/55B/61/65/77

	TLS (Authentication)
	MS6833/33A/33B/34/34B/35/55B/61/65/77

	TTLS (Authentication)
	MS6833/33A/33B/34/34B/35/55B/61/65/77

	PEAP (Authentication)
	MS6833/33A/33B/34/34B/35/55B/61/65/77


Encryption
	Features
	Comment

	TKIP (Encryption) 
	MS6833/33A/33B/34/34B/35/55B/61/65/77

	AES (Encryption)
	MS6833/33A/33B/34/34B/35/55B/61/65/77


SUPPORTED HardWAre
	Board Type
	Description

	MS6833
	802.11g miniPCI 

	MS6833A
	802.11g miniPCI 

	MS6834
	802.11g PCI

	MS6834B
	802.11g PCI

	MS6835
	802.11g Cardbus 

	MS6861
	802.11g PenType USB 2.0

	MS6865
	802.11g mini-USB 2.0

	MS6833B
	802.11g miniPCI

	MS-6855B
	802.11g+BT2.0 Combo miniPCI

	MS-6877
	802.11g mini-Card 


Installation Notes:
miniPCI/PCI/Cardbus
1. Place the hardware into PC/Laptop

2. After reboot, if System prompts “New Hardware Finding Wizard”, just click “Cancel”.

3. Double click MSI_RT6x+RT7x_XXXX.exe and fill in necessary information, setup wizard will all things for you.

USB

1. Double click MSI_RT6x+RT7x_XXXX.exe and fill in necessary information.

2. Plug-in hardware after installation

3. If system prompts “New Hardware Finding Wizard”, just click “Next” and system will automatically finish it.
Uninstall

1. Please make sure the hardware is in PC.

2. Select uninstall in “Start” => “Programs” => “MSI wireless”
3. Select “Remove all” and uninstall program will finish it automatically.

Configuration Notes:
After uninstall this driver, if you want to install again, please reboot computer, or select “Scan for handware changes “ in “Computer Management”=>”Device Manager” , if System prompts “New Hardware Finding Wizard”, just click “Cancel”.
Changes and Enhancements:
1.0.0.0302
1. Add Support for RT7x. 
2. When running RT7x, don’t copy SoftAP document to speed up installation process.
3. Add “Select utility tools” and “Select TxBurst” dialog in installer.
4. Update RT7X/RT6X and Aegis driver.
Limitations:
1. Don’t support SoftAP function in XP64bit OS.
2. USB Cards don’t support SoftAP function.
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